[EN] Before upgrading the head unit, please, make sure that the device is turned off and connected to the power supply.

1) Move the update file to a flash card or SD card with FAT32 file system;
2) Connect the card with the file to the head unit, turn on the head unit;
3) Wait for the head unit to turn on and then turn off completely (screen and button areas will off, too);
4) Remove the card from the head unit;
5) Turn on the head unit - done!

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - 

[RU] Перед обновлением, пожалуйста, проверьте, чтобы головное устройство было выключено и подключено к источнику питания.

1) Файл с прошивкой перенесите на флеш-карту или SD-карту с файловой системой FAT32;
2) Подключите карту с файлом к головному устройству, включите головное устройство;
3) Дождитесь, пока ГУ включится и снова погаснет полностью (области экрана и кнопок);
4) Извлеките флеш/SD - карту из головного устройства;
5) Включите устройство - готово!